set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d20d0030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 13
target crc val: 13=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D20D0030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d2CUSTOM_ID: 47 20 00 00 00 00 D0 03 
MAC AP : DA-F1-5B-F8-03-D2
MAC STA: D8-F1-5B-F8-03-D2
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d20d0030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 13
target crc val: 13=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D20D0030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d2CUSTOM_ID: 47 20 00 00 00 00 D0 03 
MAC AP : DA-F1-5B-F8-03-D2
MAC STA: D8-F1-5B-F8-03-D2
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d20d0030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 13
target crc val: 13=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D20D0030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d2CUSTOM_ID: 47 20 00 00 00 00 D0 03 
MAC AP : DA-F1-5B-F8-03-D2
MAC STA: D8-F1-5B-F8-03-D2
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d20d0030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 13
target crc val: 13=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D20D0030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d2CUSTOM_ID: 47 20 00 00 00 00 D0 03 
MAC AP : DA-F1-5B-F8-03-D2
MAC STA: D8-F1-5B-F8-03-D2
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d20d0030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 13
target crc val: 13=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D20D0030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d2CUSTOM_ID: 47 20 00 00 00 00 D0 03 
MAC AP : DA-F1-5B-F8-03-D2
MAC STA: D8-F1-5B-F8-03-D2
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: b9090030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 9
target crc val: 9=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:B9090030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 b9CUSTOM_ID: 47 20 00 00 00 00 90 03 
MAC AP : DA-F1-5B-F8-03-B9
MAC STA: D8-F1-5B-F8-03-B9
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.2 seconds (89.3 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 8fec0030
0x3ff00054: 0200f7b3
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 236
target crc val: 236=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:8FEC0030
    
REG1:0200F7B3
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b3 8fCUSTOM_ID: 47 20 00 00 00 0E C0 03 
MAC AP : DA-F1-5B-F7-B3-8F
MAC STA: D8-F1-5B-F7-B3-8F
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.0 seconds (89.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.5 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 8fec0030
0x3ff00054: 0200f7b3
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 236
target crc val: 236=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:8FEC0030
    
REG1:0200F7B3
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b3 8fCUSTOM_ID: 47 20 00 00 00 0E C0 03 
MAC AP : DA-F1-5B-F7-B3-8F
MAC STA: D8-F1-5B-F7-B3-8F
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 8fec0030
0x3ff00054: 0200f7b3
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 236
target crc val: 236=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:8FEC0030
    
REG1:0200F7B3
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b3 8fCUSTOM_ID: 47 20 00 00 00 0E C0 03 
MAC AP : DA-F1-5B-F7-B3-8F
MAC STA: D8-F1-5B-F7-B3-8F
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.0 seconds (89.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: dd0c0030
0x3ff00054: 0200f792
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 12
target crc val: 12=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:DD0C0030
    
REG1:0200F792
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 92 ddCUSTOM_ID: 47 20 00 00 00 00 C0 03 
MAC AP : DA-F1-5B-F7-92-DD
MAC STA: D8-F1-5B-F7-92-DD
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: dd0c0030
0x3ff00054: 0200f792
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 12
target crc val: 12=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:DD0C0030
    
REG1:0200F792
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 92 ddCUSTOM_ID: 47 20 00 00 00 00 C0 03 
MAC AP : DA-F1-5B-F7-92-DD
MAC STA: D8-F1-5B-F7-92-DD
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: fefe0030
0x3ff00054: 0200f7b6
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 254
target crc val: 254=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:FEFE0030
    
REG1:0200F7B6
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b6 feCUSTOM_ID: 47 20 00 00 00 0F E0 03 
MAC AP : DA-F1-5B-F7-B6-FE
MAC STA: D8-F1-5B-F7-B6-FE
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.com closed
set STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Trueset STOP FLG: True CONNECT BAUD: 115200
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: dd0c0030
0x3ff00054: 0200f792
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 12
target crc val: 12=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:DD0C0030
    
REG1:0200F792
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 92 ddCUSTOM_ID: 47 20 00 00 00 00 C0 03 
MAC AP : DA-F1-5B-F7-92-DD
MAC STA: D8-F1-5B-F7-92-DD
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Trueset STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d1850030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 133
target crc val: 133=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D1850030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d1CUSTOM_ID: 47 20 00 00 00 08 50 03 
MAC AP : DA-F1-5B-F8-03-D1
MAC STA: D8-F1-5B-F8-03-D1
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS
set STOP FLG: True
Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.com closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d1850030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 133
target crc val: 133=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D1850030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d1CUSTOM_ID: 47 20 00 00 00 08 50 03 
MAC AP : DA-F1-5B-F8-03-D1
MAC STA: D8-F1-5B-F8-03-D1
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.0 seconds (89.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: fefe0030
0x3ff00054: 0200f7b6
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 254
target crc val: 254=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:FEFE0030
    
REG1:0200F7B6
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b6 feCUSTOM_ID: 47 20 00 00 00 0F E0 03 
MAC AP : DA-F1-5B-F7-B6-FE
MAC STA: D8-F1-5B-F7-B6-FE
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 79910030
0x3ff00054: 0200f7a1
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 145
target crc val: 145=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:79910030
    
REG1:0200F7A1
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 a1 79CUSTOM_ID: 47 20 00 00 00 09 10 03 
MAC AP : DA-F1-5B-F7-A1-79
MAC STA: D8-F1-5B-F7-A1-79
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 15880030
0x3ff00054: 0200f7b7
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 136
target crc val: 136=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:15880030
    
REG1:0200F7B7
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b7 15CUSTOM_ID: 47 20 00 00 00 08 80 03 
MAC AP : DA-F1-5B-F7-B7-15
MAC STA: D8-F1-5B-F7-B7-15
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.0 seconds (89.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.2 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: d20d0030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 13
target crc val: 13=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:D20D0030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 d2CUSTOM_ID: 47 20 00 00 00 00 D0 03 
MAC AP : DA-F1-5B-F8-03-D2
MAC STA: D8-F1-5B-F8-03-D2
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
