set STOP FLG: True CONNECT BAUD: 115200
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 31b30030
0x3ff00054: 0200f791
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 179
target crc val: 179=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:31B30030
    
REG1:0200F791
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 91 31CUSTOM_ID: 47 20 00 00 00 0B 30 03 
MAC AP : DA-F1-5B-F7-91-31
MAC STA: D8-F1-5B-F7-91-31
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.7 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.3 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.2 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 31b30030
0x3ff00054: 0200f791
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 179
target crc val: 179=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:31B30030
    
REG1:0200F791
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 91 31CUSTOM_ID: 47 20 00 00 00 0B 30 03 
MAC AP : DA-F1-5B-F7-91-31
MAC STA: D8-F1-5B-F7-91-31
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: cfa80030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 168
target crc val: 168=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:CFA80030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 cfCUSTOM_ID: 47 20 00 00 00 0A 80 03 
MAC AP : DA-F1-5B-F8-03-CF
MAC STA: D8-F1-5B-F8-03-CF
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: ce270030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 39
target crc val: 39=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:CE270030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 ceCUSTOM_ID: 47 20 00 00 00 02 70 03 
MAC AP : DA-F1-5B-F8-03-CE
MAC STA: D8-F1-5B-F8-03-CE
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.6 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.0 seconds (89.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 1f1d0030
0x3ff00054: 0200f7be
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 29
target crc val: 29=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:1F1D0030
    
REG1:0200F7BE
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 be 1fCUSTOM_ID: 47 20 00 00 00 01 D0 03 
MAC AP : DA-F1-5B-F7-BE-1F
MAC STA: D8-F1-5B-F7-BE-1F
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.2 seconds (89.3 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.3 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 2b5b0030
0x3ff00054: 0200f7be
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 91
target crc val: 91=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:2B5B0030
    
REG1:0200F7BE
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 be 2bCUSTOM_ID: 47 20 00 00 00 05 B0 03 
MAC AP : DA-F1-5B-F7-BE-2B
MAC STA: D8-F1-5B-F7-BE-2B
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.7 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 81f90030
0x3ff00054: 0200f7b3
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 249
target crc val: 249=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:81F90030
    
REG1:0200F7B3
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b3 81CUSTOM_ID: 47 20 00 00 00 0F 90 03 
MAC AP : DA-F1-5B-F7-B3-81
MAC STA: D8-F1-5B-F7-B3-81
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.6 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 64140030
0x3ff00054: 0200f7bb
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 20
target crc val: 20=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:64140030
    
REG1:0200F7BB
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 bb 64CUSTOM_ID: 47 20 00 00 00 01 40 03 
MAC AP : DA-F1-5B-F7-BB-64
MAC STA: D8-F1-5B-F7-BB-64
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.3 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: cba60030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 166
target crc val: 166=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:CBA60030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 cbCUSTOM_ID: 47 20 00 00 00 0A 60 03 
MAC AP : DA-F1-5B-F8-03-CB
MAC STA: D8-F1-5B-F8-03-CB
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
