set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: aa380030
0x3ff00054: 0200f7bb
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 56
target crc val: 56=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:AA380030
    
REG1:0200F7BB
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 bb aaCUSTOM_ID: 47 20 00 00 00 03 80 03 
MAC AP : DA-F1-5B-F7-BB-AA
MAC STA: D8-F1-5B-F7-BB-AA
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.0 seconds (89.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.3 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 06830030
0x3ff00054: 0200f7bb
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 131
target crc val: 131=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:06830030
    
REG1:0200F7BB
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 bb 06CUSTOM_ID: 47 20 00 00 00 08 30 03 
MAC AP : DA-F1-5B-F7-BB-06
MAC STA: D8-F1-5B-F7-BB-06
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.5 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.3 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: c0320030
0x3ff00054: 0200f803
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 50
target crc val: 50=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:C0320030
    
REG1:0200F803
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f8 03 c0CUSTOM_ID: 47 20 00 00 00 03 20 03 
MAC AP : DA-F1-5B-F8-03-C0
MAC STA: D8-F1-5B-F8-03-C0
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (90.9 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.2 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: a4b60030
0x3ff00054: 0200f7ad
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 182
target crc val: 182=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:A4B60030
    
REG1:0200F7AD
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 ad a4CUSTOM_ID: 47 20 00 00 00 0B 60 03 
MAC AP : DA-F1-5B-F7-AD-A4
MAC STA: D8-F1-5B-F7-AD-A4
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.3 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (90.8 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.5 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Trueset STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
set STOP FLG: Truecom closed
set state: ESP_DL_STOP
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 79a10030
0x3ff00054: 0200f7b6
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 161
target crc val: 161=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:79A10030
    
REG1:0200F7B6
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 b6 79CUSTOM_ID: 47 20 00 00 00 0A 10 03 
MAC AP : DA-F1-5B-F7-B6-79
MAC STA: D8-F1-5B-F7-B6-79
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.5 seconds (90.4 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.5 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.3 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.8 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.6 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 82100030
0x3ff00054: 0200f7ca
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 16
target crc val: 16=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:82100030
    
REG1:0200F7CA
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 ca 82CUSTOM_ID: 47 20 00 00 00 01 00 03 
MAC AP : DA-F1-5B-F7-CA-82
MAC STA: D8-F1-5B-F7-CA-82
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.1 seconds (89.4 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Leaving...com closed
set STOP FLG: True CONNECT BAUD: 115200
com port closedset state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
0x3ff00050: 89400030
0x3ff00054: 0200f7d3
0x3ff00058: 7200b000
0x3ff0005c: 04d8f15b
check_err_0: 0bcheck_err_1: 00check_err_2: 00check_err_3: 02check_err_4: 0b====================
EFUSE NORMAL MODE
====================
=========================
CRC IN MODE 1: 
crc_calc_res: 114
target crc val: 114
=========================
=========================
CRC IN MODE 1:
crc_calc_res: 64
target crc val: 64=========================
==================
EFUSE LOG:
======================
    
EFUSE LOG:
    
---------------
    
REG0:89400030
    
REG1:0200F7D3
    
REG2:7200b000
    
REG3:04D8F15B
    
----------------
    
====================
                                   
EFUSE NORMAL MODE
                                   
====================

EFUSE CHECK PASS...48bit mac
-----------------------
 d8 f1 5b f7 d3 89CUSTOM_ID: 47 20 00 00 00 04 00 03 
MAC AP : DA-F1-5B-F7-D3-89
MAC STA: D8-F1-5B-F7-D3-89
get mac res: 1
get flash id : 0x001540a1manufacturer_id: 0xa1

device_id: 0x4015

SET FLASH PARAMS

Wrote 16384 bytes at 0x00000000 in 1.4 seconds (91.0 kbit/s)...Hash of data verified.
Wrote 425984 bytes at 0x00001000 in 38.0 seconds (89.6 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x000fe000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fc000 in 1.4 seconds (91.7 kbit/s)...Hash of data verified.
Wrote 16384 bytes at 0x001fe000 in 1.4 seconds (91.1 kbit/s)...Hash of data verified.
Leaving...com closed
